 MFAG - The Grove, Western and North Flood Alleviation Project
To prevent ground and surface water flooding the rear gardens at the afore mentioned properties in an attempt to divert surface water from entering the foul water system through rainwater down pipes and gullies and or manhole covers.
De-silt existing LLFA drainage ditch to the north of no.17 The Grove (old chapel) =£ 330.00seperate
Replace stock proof  sheep wire with barbed wire fencing 1.125m high complete with fixings to end and straining posts with straining struts, intermediate posts at 2.4 centres  64m=    
Open up & Excavate LLFA old ditch, piped and filled in 50 years ago, in the garden of 17 The Grove
Repipe newly formed trench lined with geotex  approx 1.2m -1.5m deep using, 300mm dia UPVC perforated double skinned land drainage pipes, surrounded and covered with 40mm clean stone  or clean river stones  300mm thick 40m long.  All at 1:100 fall
Backfill drainage trench and make good to garden orchard remove surplus excavated spoil from site.
Form outfall wall to 300mm dia pipe 1.250m high in local rubble stone                               
Excavate new drainage trench through cultivated flower and shrub beds approx 1.2- 1.35m deep, line trench with geotex.
Lay 300diam pipes abd  in trench and covered with stone abd, 30m long
Backfill drainage trench and make good and reinstate garden and plants, remove surplus excavated spoil from site
Form manhole inspection chamber complete with all benching and ironwork cover 1.35m deep
Form manhole inspection chamber complete with all benching and h d ironwork cover 1.2m deep
Excavate new flood alleviation drain trench approx 900-750mm deep, lined with geotex lay 225mm dia  UPVC perforated double skinned land drainage pipe to form french drain surrounded and covered with 40mm clean stone or river stones 525mm thick. Top covered with geotex matting and left open.   Surplus excavated spoil to be used to form earth bund along the boundary line between the private properties and the agricultural field, behind 1-16 The Grove. 140m long 
Excavate new flood alleviation drainage ditch450mm wide with sloped sides approx750-300mm deep, 900mm wide; to the rear of 1The Grove garden and The Coppins. 40m long
Form head wall to 225mm dia drain pipe 750mm high in local rubble stone.
Form stock proof sheep wire and barbed wire fencing 1.125m high and 45m long complete with fixings to end, return and straining posts with straining struts and intermediates at 2.4m centres.    
Total cost £16,218.00; Allow for Contingencies £ 1,621.00; Allow Administration £ 842.00
Total sum £ 18,680.00 subject to VAT at standard rate
    
